lwIP 2.2.1 Lightweight IP stack

Data Structures | Macros | Functions
dns.c File Reference
`#include "lwip/opt.h"`
`#include "lwip/def.h"`
`#include "lwip/udp.h"`
`#include "lwip/mem.h"`
`#include "lwip/memp.h"`
`#include "lwip/dns.h"`
`#include "lwip/prot/dns.h"`
`#include <string.h>`

## Data Structures
struct | dns_query
struct | dns_answer
struct | dns_table_entry
struct | dns_req_entry

## Macros
#define | DNS_RAND_TXID LWIP_RAND
#define | DNS_PORT_ALLOWED(port) ((port) >= 1024)
#define | DNS_MAX_TTL 604800

## Functions
void | dns_init (void)
void | dns_setserver (u8_t numdns, const ip_addr_t *dnsserver)
const ip_addr_t * | dns_getserver (u8_t numdns)
void | dns_tmr (void)
err_t | dns_gethostbyname (const char *hostname, ip_addr_t *addr, dns_found_callback found, void *callback_arg)
err_t | dns_gethostbyname_addrtype (const char *hostname, ip_addr_t *addr, dns_found_callback found, void *callback_arg, u8_t dns_addrtype)

## Detailed Description

DNS - host name to IP address resolver.

## Macro Definition Documentation

## ◆ DNS_MAX_TTL

#define DNS_MAX_TTL 604800

DNS resource record max. TTL (one week as default)

## ◆ DNS_PORT_ALLOWED

#define DNS_PORT_ALLOWED | ( |  | port | ) | ((port) >= 1024)

Limits the source port to be >= 1024 by default

## ◆ DNS_RAND_TXID

#define DNS_RAND_TXID LWIP_RAND

Random generator function to create random TXIDs and source ports for queries

## Function Documentation

## ◆ dns_init()

void dns_init | ( | void |  | ) |

Initialize the resolver: set up the UDP pcb and configure the default server (if DNS_SERVER_ADDRESS is set).

## ◆ dns_tmr()

void dns_tmr | ( | void |  | ) |

The DNS resolver client timer - handle retries and timeouts and should be called every DNS_TMR_INTERVAL milliseconds (every second by default).